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Description automatically generated with low confidence]                                                Tripoli Southern Highlands #155            Flight Card

	Name:     
	Date:

	Phone:     
	S. Clearance No: 

	TRA #:      
	Cert Level:     
	Pyro Licence No: 

	Rocket Name:
	Weight (g):

	Colour:
	*Stability:
	Stages:
	Est. Altitude:

	Flight Info:
 Cert – Level __
 RTF Model
 Kit Built
 Modified Kit (*)
 Scratch Built (*)
 Other                                 
	Motor Configuration
	Recovery Info:
	Telemetry:
  Yes  No
Freq: ______ MHz
GPS/Tracker:
  Yes  No

	
	Qty
	Type
	Delay
	  Motor       Electronic
	

	
	
	
	
	  Dual-deploy @ _____ ft
	

	
	
	
	
	  Chute       Streamer
	

	
	
	
	
	  Glider       Tumble
	

	
	 Motor Type:     Black Powder     Composite     Cluster     Water                                                                                           
  Hybrid     Staged      Sparky (Advise RSO & LCO prior to launch session)

	This section for RSO/LCO use only             HPR         LPR          RSO initial:

	Pre-flight:
	Flight outcome:
	Bank #

Pad #

	Waiver Signed? Yes  No
CoG/CoP OK?  Yes  No
Structure OK?    Yes  No
Flown before?   Yes  No
	  Good
  CATO
  Ballistic
 Other:
	  Unstable
  Break-up
  Lost
	 Tangled
 Strip
 No Flight

	

	Wind
Speed:
	Notes:
	LCO 
initial:
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CRG Flight Card Instructions
Please complete a flight card for each flight.  These cards provide the Range Safety Officer (RSO) with the details necessary for assessing the safety of the flight vehicle, and for coordination of the launch by the Launch Control Officer (LCO).
Prior to Check-in with the RSO:
· Complete all sections (as applicable) – do not write in the grey section
· Ready the rocket for flight, including loading the motor, but DO NOT insert the igniter/s
· Shunt (short together) all charge leads if electrical deployment systems used
· Assess the CoG of the rocket and ensure a stability margin exists against the CoP – the RSO will ask you about this. * For modified kits and scratch builds, please confirm how you assessed the stability.
At the RSO table:
· Present the completed flight card, rocket and any other relevant info (i.e., motor data sheet, sim printouts etc).
· When checked and accepted for flight, the RSO will assign a pad number
At the LCO table:
· Present the Flight Card, and when the Range is OPEN, proceed to set-up on the assigned pad.
· When set up, or when requested, return to the LCO, advise READY or NOT READY
	Sponsored Launch Information 
A sponsored launch will normally be supervised by a CRG committee member, or a suitably certified ordinary member appointed by the committee.

Launch Supervisor:                                             UHL No:                        XPYR No:
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